**AZ-M30
High Definition Borescope Inspection Camera**

**Applications**
- Medical use
- Human examination

**Features**
- High performance industrial inspection camera with a 3-inch high definition colour LCD.
- It is ergonomically designed so that the main functional buttons can be controlled with one hand.
- The snapshot and recording functions are supported, photos and videos can be saved on TF memory card.
- Auxiliary light source and adjustable LED lights making it easy and handy to use in a dark environment.

|  |
| --- |
| **Specifications** |
| Screen | 3.0inch color LCD display (1080p) |
| Resolution | 1920\*1080 |
| Horizontal viewing angle | 60° |
| Video Output Format | NTSC |
| Image Size | Images – size (1270X 1080) and format (JPG) |
| Video Size | (1920 X 1080 and format (AVI) |
| SD Card | 4G Included (supports up to 64G) |
| Line length | 2M |
| Focal length | 1.2” to 4.0” (3cm-10cm) |
| Waterproof level | IP67(only for camera head and lens) |
| Lens diameter | 5.5mm |
| Battery capacity | 3000mAh |
| Battery life | Approximately 3-4 hours |
| Dimensions | 9.0\*6.7\*3.0” (23CM\*17CM\*8CM) |
| Weight | 1.8lb (0.8kg) |